# GENERAL

## Summary

### Comply with the requirements of Division 1 - General Requirements.

### This Specification Section covers the requirements for supplying, placing, maintaining, and removing support systems required to permit the excavation and backfilling of trenches or excavations for the installation of sanitary and storm pipe sewers, pipe culverts and end sections, forcemains and associated appurtenances, watermains and associated appurtenances, and other underground Utilities; maintenance holes, catch basins, ditch inlets, and valve chambers; and any other specified subsurface construction.

## Related Sections

#### Section 02511 – Watermains

#### Section 02530 ­– Sewerage

#### Section 02531 – Sewage Forcemains

#### Section 02631 – Manholes and Catchbasins

## References

### Ontario Provincial Standards for Roads and Public Works

#### OPSS.MUNI 404 Support Systems (Nov 2017)

### Occupational Health and Safety Act, R.S.O. 1990, c.O.1, as amended

### Ontario Regulation 213/91 Construction Projects, as amended

## Definitions

### OPSS.MUNI 404.03 shall be followed

## Design and Submission Requirements

### OPSS.MUNI 404.04.01.01 shall be followed.

## Measurement and Payment

### All costs associated with the work of this Section shall be included in the price for Item No. A2.01 in the Bid Form.

# MATERIALS (Not used)

# EXECUTION

## OPSS.MUNI 404.07 shall be followed with the following amendments:

**404.07.03** **Removal, Backfilling and Compacting** is amended by the replacement of the first paragraph with the following:

As the excavation is backfilled, the support system shall be removed, unless it is specified in the Contract Documents to be left in place or approved by the Consultant.

**END OF SECTION**