|  |  |  |
| --- | --- | --- |
| Version | Date | Description of Revisions |
| 1 | August 30, 2006 | Approved final document. |
| 2 | September 28, 2010 | Minor revisions |
| 3 | June 10, 2014 | Review comments (AV) |
| 4 | June 8, 2015 | Second Draft for Review (AV) |
| **5** | **September 16, 2015** | **Updated, Finalized Specification – Reference eDOCS #5823644-v4 (AV)** |
| 6 | May 18, 2017 | Updated reference standard ASTM D2855-15 (AAM) |

NOTE:

This is a CONTROLLED Document. Any documents appearing in paper form are not controlled and should be checked against the on-line file version prior to use.

**Notice:** This Document hardcopy must be used for reference purpose only.

**The on-line copy is the current version of the document.**

## References

### ASTM

#### [ASTM D2665-14, Standard Specification for Poly(Vinyl Chloride) (PVC) Plastic Drain, Waste, and Vent Pipe and Fittings](http://www.astm.org/Standards/D2665.htm)

#### ASTM D2564-12, Standard Specification for Solvent Cements for Poly(Vinyl Chloride) (PVC) Plastic Piping Systems

#### ASTM D1784-11, [Standard Specification for Rigid Poly(Vinyl Chloride) (PVC) Compounds and Chlorinated Poly(Vinyl Chloride) (CPVC) Compounds](http://www.astm.org/Standards/D1784.htm)

#### ASTM D2855-15 [Standard Practice for Making Solvent-Cemented Joints with Poly(Vinyl Chloride) (PVC) Pipe and Fittings](http://www.astm.org/Standards/D2855.htm)

### ANSI/NSF

#### ANSI/NSF 14 – 2012, Plastics Piping System Components and Related Materials

|  |  |  |
| --- | --- | --- |
| Item | Size | Description |
| Pipe and Fittings | All | PVC-DWV Schedule 40 non-pressure application, Class 12454B conforming to the requirements of ASTM D2665-14 and ANSI/NSF Standard 14 system. |
| Joints | All | Solvent cemented conforming to the requirements of ASTM D2855-15 except where connection to equipment may require future removal. |
| Solvent Cement | All | As recommended by the pipe and fitting manufacturer conforming to the requirements of ASTM D2564-12, ASTM D1784-11 and ASTM D2855-15. |

**END OF SECTION**