# GEneral

## Summary

### This Section includes the general requirements for the retention of a specialty subcontractor who shall perform dewatering in accordance with Permission To Take Water (PTTW) conditions.

## Related Sections

#### Section 01060 – Regulatory Requirements

#### Section 01300 – Submittals

#### Section 01561 – Environmental Protection

#### Section 02230 – Site Preparation for Pipelines, Utilities and Associated Structures

#### Section 02240 – Dewatering- General

#### Section 02241 – Provide Water Control Plan, Dewatering, Discharge Plan and Groundwater Monitoring Program

#### Section 02242 – Supply Install and Subsequently Remove Dewatering System

#### Section 02243 – Operate and Maintain Dewatering System

#### Section 02244 – Retain Specialty Subcontractor To Monitor Groundwater Levels And Discharge Water Quality

#### Section 02315 – Trenching, Backfilling and Compacting

## References

### Ontario Ministry of the Environment and Climate Change website

#### <http://www.ontario.ca/page/permits-take-water>

### Ontario Provincial Standards for Roads and Public Works (OPSS)

#### OPSS 492 (November 2010) Site Restoration Following Installation Of Pipelines, Utilities And Associated Structures

#### OPSS.MUNI 517 (Apr 2017) Dewatering of Pipeline, Utility and Associated Structure Excavation

#### OPSS.MUNI 518 (Apr 2017) Control of Water From Dewatering Operations

### Ontario Water Resources Act R.S.O. 1990 c. O.40

#### O. Reg. 387/04 Water Taking and Transfer R.R.O. 1990, Reg. 903: Wells

### Regional Municipality of York

#### Bylaw 2014-23 Discharge of Sewage, Storm Water and Land Drainage Bylaw (Amended 2014)

## Measurement and Payment

### All costs associated with the work of this Section shall be included in the price(s) for Item No(s). A2.04 in the Bid Form.

# PRODUCTS (Not Used)

# EXECUTION

## General

### The Contractor shall perform restoration works associated with dewatering activities (including but not limited to, removal and disposal of dewatering and decommissioning of monitoring wells, placing topsoil, sod, asphalt as required) to restore the Site to its pre-construction condition or better.

### Payment for the work of this Section under Item No. A2.04 of the Bid Form shall be paid in accordance with the percentage of work under this Section that has been completed as estimated by the Consultant in its sole discretion.

**END OF SECTION**