|  |  |  |
| --- | --- | --- |
| Version | Date | Description of Revisions |
| 1 | August 30, 2006 | Approved final document. |
| 2 | June 10, 2014 | First draft review comments (AV) |
| 3 | June 8, 2015 | Second Draft for Review (AV) |
| **4** | **September 16, 2015** | **Updated, Finalized Specification – Reference eDOCS #5823646-v4 (AV)** |

NOTE:

This is a CONTROLLED Document. Any documents appearing in paper form are not controlled and should be checked against the on-line file version prior to use.

**Notice:** This Document hardcopy must be used for reference purpose only.

**The on-line copy is the current version of the document.**

## References

### American Society for Testing Materials (ASTM)

#### [ASTM A518/A518M-99(2012), Standard Specification for](http://www.astm.org/Standards/D2665.htm) Corrosion-Resistant High-Silicon Iron Castings

#### ASTM A861-04(2013), Standard Specification for High-Silicon Iron Pipe and Fittings

|  |  |  |
| --- | --- | --- |
| Item | Size | Description |
| Pipe and Fittings | All | High silicone cast iron, no-hub ends, extra heavy grade, conforming to ASTM A518/A518M-99(2012) and ASTM A861-04(2013). |
| Joints | All | No-hub type compression coupling, with Teflon inner sleeve, neoprene outer sleeve, and stainless steel shield and clamp assembly. |

**END OF SECTION**