|  |  |  |
| --- | --- | --- |
| Version | Date | Description of Revisions |
| 1 | September 21, 2009 | Excel Form Created |
| 2 | September 22, 2015 | Conversion of form into MSWord |
|  |  |  |
|  |  |  |
|  |  |  |

NOTE:

This is a CONTROLLED Document. Any documents appearing in paper form are not controlled and should be checked against the on-line file version prior to use.

**Notice:** This Document hardcopy must be used for reference purpose only.

**The on-line copy is the current version of the document.**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Symbol: | | | | |  |  |  |  |
| Area Served | | | | |  |  |  |  |
| Indoor  Fan  Data | Supply Air | | L/s | |  |  |  |  |
| Outside Air | | L/s | |  |  |  |  |
| External Static Pressure | | kPa | |  |  |  |  |
| kW | | | |  |  |  |  |
| Voltage | | | |  |  |  |  |
| Phase | | | |  |  |  |  |
| DX Cooling Data | Total | | kW | |  |  |  |  |
| Sens. | | kW | |  |  |  |  |
| Entering Air Temp. | DB | oC | |  |  |  |  |
| WB | oC | |  |  |  |  |
| Ambient Temp | | oC | |  |  |  |  |
| Compressor Data | No. | | | |  |  |  |  |
| Steps | | | |  |  |  |  |
| RLA (ea.) | | | |  |  |  |  |
| LRA (ea.) | | | |  |  |  |  |
| Voltage | | | |  |  |  |  |
| Phase | | | |  |  |  |  |
| Condenser Fan Data | No. | | | |  |  |  |  |
| kW (ea.) | | | |  |  |  |  |
| Voltage | | | |  |  |  |  |
| Phase | | | |  |  |  |  |
| L/s (Total) | | | |  |  |  |  |
| Electrical  Data | # of Connections | | | |  |  |  |  |
| MCA | | | |  |  |  |  |
| MCOP (Fuse) | | | |  |  |  |  |
| Voltage | | | |  |  |  |  |
| Phase | | | |  |  |  |  |
| Dimensions | Width | | | m |  |  |  |  |
| Depth | | | m |  |  |  |  |
| Height | | | m |  |  |  |  |
| Maximum Weight | | | kg |  |  |  |  |
| Manufacturer: | | | | |  |  |  |  |
| Model No: | | | | |  |  |  |  |
| Applicable Remarks: | | | | |  |  |  |  |
| Remarks:   |  |  |  |  | | --- | --- | --- | --- | | **A:** | Condenser Coil Shall Have Dip Applied Anti-Corrosion Coating (Not Spray Applied) | **E:** | 2-Inch Deep Pleated Air Filter Sized To Suit Return Grille | | **F:** | Factory Installed Disconnect | | **B:** | Double Deflection Supply Grille, Titus 272rs Or Equal, Sized To Suit Supply Air Opening | **G:** | Fresh Air Damper | | **H:** | Desert Duty Kit | | **C:** | Filter Back Return Grille, Titus 33rfl Or Equal, Sized To Suit Return Air Opening | **I:** | Cold Weather Kit | | **J:** | Dehumidification Package | | **D:** | 5-Year Compressor Warranty | **K:** | Hot Gas Bypass | | | | | | | | | |